Hi Terry,

Here are the specific reporting requirements for AHRI certification:

* **Initial Report**: Within 5 minutes after DR event reception
* **Interval Reports**: Every 15 minutes by default (or as specified by VTN)
* **Final Report**: Within 5 minutes after DR event ends

Both report types are required when requested by the VTN – [1] Device Status Reports (individual device data) [2] Aggregate Reports (total load reduction metrics)

The VTN determines which report type(s) it needs during testing, and our system must be able to provide both. We have to create both reports, and we cannot choose to implement only one type.

Here’s a flowchart.

